1. Read for key press
   1. If key is pressed, move single motor in specified direction
   2. Each key maps to one motor in one direction
   3. 6 keys total for CW + CCW for 3 motors
2. When key is not pressed, motor should be off
3. Track rotation of each motor
   1. Can press another key to reset all motors