1. Read for key press
   1. If key is pressed, move single motor in specified direction
   2. Each key maps to one motor in one direction
   3. 6 keys total for CW + CCW for 3 motors
2. When key is not pressed, motor should be off
3. Track rotation of each motor
   1. Can press another key to reset all motors
4. Set up key mapping as a variable array to easily change later